DS – generates a sine wave, pick the frequency, 9 kHz = DDS front end = on the other side it has a transimpedance amplifier,

Goertzal algorithm